# Classes::Vms

Project: Classes | Vms : Public <<D2Class>> Class
Created: | 26/02/2020 20:59:41
Modified: | 29/11/2022 17:26:12
Project: |
Author: |
Version: | 1.0
Phase: | 1.0
Status: | Proposed
Complexity: | Easy
Difficulty: |
Priority: |
Multiplicity: |
Advanced: |
UUID: | {D415FCCA-2BF4-4e34-912E-43CF6360602F}
Appears In: | VmsTablePublication
Attributes Associations To Associations From Tagged Values Advanced Other Links
Attribute | Scope | Type
dedicatedUsage | Public | DedicatedUsageEnum
definition=Type of usage to which this VMS is dedicated order=11
description | Public | MultilingualString
definition=The description of the VMS (possibly giving a description of its location or its normal use). order=1
displayHeight | Public | MetresAsFloat
definition=Height in metres of the sign's overall display area. order=8
displayWidth | Public | MetresAsFloat
definition=Width in metres of the sign's overall display area. order=9
dynamicallyConfigurable | Public | Boolean
definition=Identifies (when True) that the VMS has a display area that may be dynamically configured to display different combinations of text and pictogram areas. The current configuration will normally be given with each published current VMS setting. order=7
heightAboveCarriageway | Public | MetresAsFloat
definition=Height in metres of the mounted sign above the carriageway, measured to the bottom of the display area. order=10
lanternsPresent | Public | Boolean
definition=Indicates whether the VMS is equipped with flashing lights (called lanterns in some countries) outside the text or pictogram display areas order=0
owner | Public | MultilingualString
definition=Owner (authority or organisation) of the VMS. This may not be the same as the authority or organisation which is currently controlling the VMS. order=2
physicalSupport | Public | PhysicalSupportEnum
definition=Description of how the VMS is physically mounted or deployed on the road. order=3
vmsType | Public | VmsTypeEnum
definition=Broad classification of the type of variable message sign. order=4
vmsTypeCode | Public | String
definition=Specification of the type of VMS defined by a code, normally country or even manufacturer specific (e.g. MS4). order=5
Element | Source Role | Target Role
«D2VersionedIdentifiable» VmsController Class «D2Relation» | Name: | Name:
Details:
Element | Source Role | Target Role
«D2Class» ManagedLogicalLocation Class «D2Relation» | Name: | Name:
Details:
«D2Class» VmsConfiguration Class «D2Relation» | Name: | Name:
Details:
«D2Class» Location Class «D2Relation» | Name: vmsLocation | Name:
Details:
«D2Class» UrlLink Class «D2Relation» | Name: imageLink | Name:
Details:
Tag | Value
definition | Variable message sign - a display panel used to display one or more messages (text, symbols, pictograms or combinations) that can be changed or switched on or off as required
Details:
Property | Value
isFinalSpecialization: | 0
Object | Type | Connection | Direction | Notes
«D2Class» ManagedLogicalLocation | Class | Strong | From |
«D2VersionedIdentifiable» VmsController | Class | Strong | To |
«D2Class» VmsConfiguration | Class | Strong | From |
«D2Class» Location | Class | Strong | From |
«D2Class» UrlLink | Class | Strong | From |