# Enumerations::FaultTypeEnum

Project: Enumerations | FaultTypeEnum : Public <<D2Enumeration>> Enumeration
Created: | 28/08/2017 14:44:15
Modified: | 29/11/2022 17:26:06
Project: |
Author: | Freudenstein
Version: | 1.0
Phase: | 1.0
Status: | Proposed
Complexity: | Easy
Difficulty: |
Priority: |
Multiplicity: |
Advanced: |
UUID: | {998F193C-1947-4cfb-A451-C3DB8727CA04}
Appears In: | AllFaultsOfSingleDevice
Attributes Tagged Values Advanced
Attribute | Scope | Type
internalCommunicationFault | Public | enumerationLiteral
changed=new definition=Device may be connected but has a communications fault that may prevent a required communication function performing within specified requirements. order=0 origin=- null - originalCode=- null - originalName=- null -
synchronizationFault | Public |
definition=Fault in the process of synchronisation with the device order=17
componentFault | Public | enumerationLiteral
changed=new definition=A fault located in a component of the device (other components could still work well). order=1 origin=- null - originalCode=- null - originalName=- null -
configurationError | Public | enumerationLiteral
changed=new definition=An error in the configuration or supply data of the device. order=2 origin=- null - originalCode=- null - originalName=- null -
disconnected | Public | enumerationLiteral
changed=new definition=The device or component has no connection order=3 origin=- null - originalCode=- null - originalName=- null -
electronicsFault | Public | enumerationLiteral
changed=new definition=A fault in the electronics part of the device. order=4 origin=- null - originalCode=- null - originalName=- null -
generalSystemError | Public | enumerationLiteral
changed=new definition=A general system error. order=5 origin=- null - originalCode=- null - originalName=- null -
hardwareFault | Public | enumerationLiteral
changed=new definition=A hardware-related fault. order=6 origin=- null - originalCode=- null - originalName=- null -
controlFault | Public | enumerationLiteral
changed=new definition=An invalid state was called by the control unit. order=8 origin=- null - originalCode=- null - originalName=- null -
intermittentlyWorking | Public | enumerationLiteral
changed=new definition=The device or component cannot always perform its tasks as required. order=9 origin=- null - originalCode=- null - originalName=- null -
mechanicalFault | Public | enumerationLiteral
changed=new definition=A fault of a mechanical part of the device. order=10 origin=- null - originalCode=- null - originalName=- null -
notWorking | Public | enumerationLiteral
changed=new definition=The device or component cannot perform its tasks. order=11 origin=- null - originalCode=- null - originalName=- null -
operatingSystemFault | Public | enumerationLiteral
changed=new definition=A fault in the operating system of the device. order=12 origin=- null - originalCode=- null - originalName=- null -
powerFailure | Public | enumerationLiteral
changed=new definition=There is no power supply for the device or component. order=13 origin=- null - originalCode=- null - originalName=- null -
securityFault | Public | enumerationLiteral
changed=new definition=A fault that causes a security issue or harms security related services. order=14 origin=- null - originalCode=- null - originalName=- null -
softwareFault | Public | enumerationLiteral
changed=new definition=A software-related fault. order=16 origin=- null - originalCode=- null - originalName=- null -
timeOrClockFault | Public | enumerationLiteral
changed=new definition=The device clock does not work properly or reports inconsistent time keeping. order=18 origin=- null - originalCode=- null - originalName=- null -
unspecifiedFault | Public | enumerationLiteral
changed=new definition=The fault cannot be specified. order=20 origin=- null - originalCode=- null - originalName=- null -
unknownFault | Public | enumerationLiteral
changed=new definition=The fault is unknown. order=21 origin=- null - originalCode=- null - originalName=- null -
otherFault | Public | enumerationLiteral
changed=new definition=The fault is not included in this enumeration. order=22 origin=- null - originalCode=- null - originalName=- null -
Tag | Value
changed | new
Details: Default: new
definition | This enumeration provides information on types of faults.
Details:
origin | - null -
Details: Default: - null -
originalCode | - null -
Details: Default: - null -
originalName | - null -
Details: Default: - null -
Property | Value
isFinalSpecialization: | 0