# Final::EuVehicleCategoryEnum

Project: Final | EuVehicleCategoryEnum : Public <<D2Enumeration>> Enumeration
Created: | 14/05/2019 10:43:58
Modified: | 18/02/2025 11:23:10
Project: |
Author: | Bard
Version: | 1.0
Phase: | 1.0
Status: | Proposed
Complexity: | Easy
Difficulty: |
Priority: |
Multiplicity: |
Advanced: |
UUID: | {4B1C6EF2-56C6-469d-9109-3F26E2F55AF2}
Appears In: | Enumerations
Attributes Tagged Values Advanced
Attribute | Scope | Type
l1 | Public |
definition=Light two-wheel powered vehicle. order=0
l2 | Public |
definition=Three-wheel moped. order=1
l3 | Public |
definition=Two-wheel motorcycle. order=2
l4 | Public |
definition=Two-wheel motorcycle with side-car. order=3
l5 | Public |
definition=Powered tricycle. order=4
l6 | Public |
definition=Light quadricycle. order=5
l7 | Public |
definition=Heavy quadricycle. order=6
m | Public |
definition=Motor vehicles with at least four wheels designed and constructed for the carriage of passengers. order=7
r | Public |
definition=Agricultural trailer: any agricultural or forestry vehicle intended mainly to be towed by a tractor and intended mainly to carry loads or process materials. The ratio of the techn. permissible max. laden to unladen mass is equal to or greater than 3.0. order=31
r1 | Public |
definition=Trailers, the sum of the technically permissible masses per axle of which does not exceed 1,500 kg. order=8
r2 | Public |
definition=Trailers, the sum of the technically permissible masses per axle of which exceeds 1,500 kg but does not exceed 3,500 kg. order=9
r3 | Public |
definition=Trailers, the sum of the technically permissible masses per axle of which exceeds 3,500 kg but does not exceed 21,000 kg. order=10
r4 | Public |
definition=Trailers, the sum of the technically permissible masses per axle of which exceeds 21,000 kg. order=11
t1 | Public |
definition=Wheeled tractors with the closest axle to the driver having a minimum track width of not less than 1,500 mm; with an unladen mass in running order of more than 600 kg and with a ground clearance of not more than 1,000 mm. order=12
t2 | Public |
definition=Vehicle category t2 according to Regulation (EU) No 167/2013. order=13
t3 | Public |
definition=Wheeled tractors with unladen mass in running order of not more than 600 kg. order=14
t4 | Public |
definition=Special purpose wheeled tractors with a maximum design speed of not more than 40 km/h. order=15
t41 | Public |
definition=Category T4.1: High clearance tractors. order=16
t42 | Public |
definition=Category T4.2: Extra-wide tractors. order=17
t43 | Public |
definition=Category T4.3: Low clearance tractors. order=18
m1 | Public |
definition=Vehicles designed and constructed for the carriage of passengers and comprising no more than eight seats in addition to the driver’s seat. order=19
m2 | Public |
definition=Vehicles designed and constructed for the carriage of passengers, comprising more than eight seats in addition to the driver’s seat, and having a maximum mass not exceeding 5 tonnes. order=20
m3 | Public |
definition=Vehicles designed and constructed for the carriage of passengers, comprising more than eight seats in addition to the driver’s seat, and having a maximum mass exceeding 5 tonnes. order=21
n | Public |
definition=Motor vehicles with at least four wheels designed and constructed for the carriage of goods. order=22
n1 | Public |
definition=Vehicles designed and constructed for the carriage of goods and having a maximum mass not exceeding 3,5 tonnes order=23
n2 | Public |
definition=Vehicles designed and constructed for the carriage of goods and having a maximum mass exceeding 3,5 tonnes but not exceeding 12 tonnes. order=24
n3 | Public |
definition=Vehicles designed and constructed for the carriage of goods and having a maximum mass exceeding 12 tonnes. order=25
o | Public |
definition=Trailers (including semi-trailers). order=26
o1 | Public |
definition=Trailers with a maximum mass not exceeding 0,75 tonnes order=27
o2 | Public |
definition=Trailers with a maximum mass exceeding 0,75 tonnes but not exceeding 3,5 tonnes. order=28
o3 | Public |
definition=Trailers with a maximum mass exceeding 3,5 tonnes but not exceeding 10 tonnes. order=29
o4 | Public |
definition=Trailers with a maximum mass exceeding 10 tonnes. order=30
Tag | Value
definition | Vehicle categories according to EU legislation.
Details:
regulatoryContext | EU 2007/46/EG, EU 168/2013, EU 167/2013
Details:
Property | Value
isFinalSpecialization: | 0