# Enumerations::ChargingModeEnum

Project: Enumerations | ChargingModeEnum : Public <<D2Enumeration>> Enumeration
Created: | 26/03/2021 09:13:02
Modified: | 29/11/2022 17:26:03
Project: |
Author: | Freudenstein
Version: | 1.0
Phase: | 1.0
Status: | Proposed
Complexity: | Easy
Difficulty: |
Priority: |
Multiplicity: |
Advanced: |
UUID: | {78F60CDD-4EAD-4979-81DC-43BC565B5496}
Appears In: | ElectricChargingPoint, EnergyInfrastructureTablePublication
Attributes Tagged Values Advanced
Attribute | Scope | Type
mode1AC1p | Public |
definition=Mode 1, AC 1 phase order=0
mode1AC3p | Public |
definition=Mode 1, AC 3 phases order=1
mode2AC1p | Public |
definition=Mode 2, AC 1 phase order=2
mode2AC3p | Public |
definition=Mode 2, AC 3 phases order=3
mode3AC3p | Public |
definition=Mode 3, AC 3 phases order=4
mode4DC | Public |
definition=Mode 4, DC order=5
legacyInductive | Public |
definition=Legacy-Inductive order=6
ccs | Public |
changed=new definition=Charging with a combined charging solution (CCS). AC and DC are used simultaneously. order=8 origin=- null - originalCode=- null - originalName=- null -
other | Public |
definition=Some other charging mode order=10
unknown | Public |
changed=new definition=The type of the charging mode is unknown order=11 origin=- null - originalCode=- null - originalName=- null -
Tag | Value
definition | Charging mode according to IEC 61851-1 terminology
Details:
Property | Value
isFinalSpecialization: | 0