# Enumerations::ChargingModeEnum

Project: Enumerations | ChargingModeEnum : Public <<D2Enumeration>> Enumeration
Created: | 26/03/2021 09:13:02
Modified: | 12/02/2026 12:54:52
Project: |
Author: | Freudenstein
Version: | 1.0
Phase: | 1.0
Status: | Proposed
Complexity: | Easy
Difficulty: |
Priority: |
Multiplicity: |
Advanced: |
UUID: | {C6DD2A72-CBFF-49a3-8C78-1CD39DAAB20C}
Appears In: | ElectricChargingPoint, EnergyInfrastructureTablePublication
Attributes Tagged Values Advanced
Attribute | Scope | Type
mode1AC1p | Public |
definition=Mode 1, AC 1 phase. order=0
mode1AC3p | Public |
definition=Mode 1, AC 3 phases. order=1
mode2AC1p | Public |
definition=Mode 2, AC 1 phase. order=2
mode2AC3p | Public |
definition=Mode 2, AC 3 phases. order=3
mode3AC3p | Public |
definition=Mode 3, AC 3 phases. order=4
mode4DC | Public |
definition=Mode 4, DC. order=5
legacyInductive | Public |
definition=Legacy-Inductive order=6
ccs | Public |
changed=new definition=Charging with a combined charging solution (CCS). AC and DC are used simultaneously. order=8 origin=- null - originalCode=- null - originalName=- null -
other | Public |
definition=Some other charging mode. order=10
unknown | Public |
changed=new definition=The type of the charging mode is unknown. order=11 origin=- null - originalCode=- null - originalName=- null -
Tag | Value
definition | Charging mode according to IEC 61851-1 terminology.
Details:
Property | Value
isFinalSpecialization: | 0