# Enumerations::DeviceHealthEnum

Project: Enumerations | DeviceHealthEnum : Public <<D2Enumeration>> Enumeration
Created: | 07/09/2017 16:36:25
Modified: | 29/11/2022 17:26:06
Project: |
Author: | Freudenstein
Version: | 1.0
Phase: | 1.0
Status: | Proposed
Complexity: | Easy
Difficulty: |
Priority: |
Multiplicity: |
Advanced: |
UUID: | {07CAE3F4-356B-4a8c-BA12-67129C2DA066}
Appears In: | Status
Attributes Tagged Values Advanced
Attribute | Scope | Type
ok | Public |
changed=new definition=The device is working properly according to its specified requirements. order=0 origin=- null - originalCode=- null - originalName=- null -
notOk | Public |
changed=new definition=The device is not working properly according to its specified requirements. A reference to a fault may be provided. order=1 origin=- null - originalCode=- null - originalName=- null -
functionalityPartlyOk | Public |
changed=new definition=Some specific functionality of the device is working properly according to its specified requirements, but some other is not. order=2 origin=- null - originalCode=- null - originalName=- null -
intermittentlyOk | Public |
changed=new definition=The device is sometimes working properly according to its specified requirements, but on occasions is not. A reference to a fault may be provided. order=3 origin=- null - originalCode=- null - originalName=- null -
alarm | Public |
changed=new definition=There is an indication of a fault danger or some other undesirable effects. An example might be an environmental alarm, for instance the device-temperature being above a certain threshold. order=4 origin=- null - originalCode=- null - originalName=- null -
notResponding | Public |
changed=new definition=The device does not respond on calling. Nevertheless, it can be possible that the device still sends data. Normally this information is gathered from a system trigger or log trace, which is acknowledged and recorded by an operator. order=5 origin=- null - originalCode=- null - originalName=- null -
offline | Public |
changed=new definition=The device is not connected or cannot be contacted. A reference to a fault may be provided. Usually, this information is generated by an operator. order=6 origin=- null - originalCode=- null - originalName=- null -
unknown | Public |
changed=new definition=The status of the device is unknown. order=7 origin=- null - originalCode=- null - originalName=- null -
Tag | Value
changed | new
Details: Default: new
definition | This enumeration provides information on the health status of a device, in terms of its ability to provide its functional service.
Details:
origin | - null -
Details: Default: - null -
originalCode | - null -
Details: Default: - null -
originalName | - null -
Details: Default: - null -
Property | Value
isFinalSpecialization: | 0