# Final::EuBodyworkCodeEnum

Project: Final | EuBodyworkCodeEnum : Public <<D2Enumeration>> Enumeration
Created: | 25/04/2024 10:28:56
Modified: | 18/02/2025 11:23:10
Project: |
Author: | TB
Version: | 1.0
Phase: | 1.0
Status: | Proposed
Complexity: | Easy
Difficulty: |
Priority: |
Multiplicity: |
Advanced: |
UUID: | {1B7335CF-DF30-406b-8E63-16070B311411}
Appears In: | Enumerations
Attributes Tagged Values Advanced
Attribute | Scope | Type
aa | Public |
definition=Saloon - A vehicle defined in term 3.1.1.1 of international standard ISO 3833:1977, fitted with at least four side windows. order=0
ab | Public |
definition=Hatchback - A saloon as defined in REGULATION (EU) 2018/858 Annex 1 Part C Ref. 2.1 with a hatch at the rear end of the vehicle. order=1
ac | Public |
definition=Station wagon - A vehicle defined in term 3.1.1.4 of international standard ISO 3833:1977. order=2
ad | Public |
definition=Coupé - A vehicle defined in term 3.1.1.5 of international standard ISO 3833:1977. order=3
ae | Public |
definition=Convertible - A vehicle defined in terms No 3.1.1.6 of international standard ISO 3833:1977. However, a convertible may have no door. order=4
af | Public |
definition=Multi-purpose - A vehicle other than AG and those mentioned in AA to AE in tended for carrying persons and their luggage or occasionally goods, in a single compartment. order=5
ag | Public |
definition=Truck station wagon-Vehicle defined in term No 3.1.1.4.1 of ISO 3833:1977. The luggage compartment must be compl. sepated from the passenger compartment. And the ref. point of the driver's seating pos. must be min. 750mm above the surface supp. the veh. order=6
ba | Public |
definition=Lorry - A vehicle that is designed and constructed exclusively or principally for conveying goods. It may also tow a trailer. order=7
bb | Public |
definition=Van - A lorry with the compartment where the driver is located and cargo area within a single unit. order=8
bc | Public |
definition=Tractor unit for semi-trailer - A towing vehicle that is designed and constructed exclusively or principally to tow semi-trailers. order=9
bd | Public |
definition=Road tractor - A towing vehicle that is designed and constructed exclusively to tow trailers other than semi-trailers. order=10
be | Public |
definition=Pick-up truck - A vehicle of a maximum mass not exceeding 3 500 kg in which the seating positions and the cargo area are not located in a single compartment. order=11
bx | Public |
definition=Chassis-cab or chassis-cowl - An incomplete vehicle with just a cabin (complete or partial), chassis rails, power train, axles, which is intended to be completed with bodywork, customised to the needs of the transport operator. order=12
ca | Public |
definition=Single-deck vehicle - A vehicle where the spaces provided for persons are arranged in a single level or in a way that they do not constitute two superimposed levels. order=13
cb | Public |
definition=Double-deck vehicle - A vehicle defined in paragraph 2.1.6 of UN Regulation No 107. order=14
cc | Public |
definition=Single-deck articulated vehicle - A vehicle defined in paragraph 2.1.3 of UN Regulation No 107 with a single deck. order=15
cd | Public |
definition=Double-deck articulated vehicle - A vehicle defined in paragraph 2.1.3.1 of UN Regulation No 107. order=16
ce | Public |
definition=Low-floor single-deck vehicle - A vehicle defined in paragraph 2.1.4 of UN Regulation No 107 with a single deck. order=17
cf | Public |
definition=Low-floor double-deck vehicle - A vehicle defined in paragraph 2.1.4 of UN Regulation No 107 with a double deck. order=18
cg | Public |
definition=Articulated low-floor single-deck vehicle - A vehicle that combines the technical features of codes CC and CE. order=19
ch | Public |
definition=Articulated low-floor double-deck vehicle - A vehicle that combines the technical features of codes CD and CF. order=20
ci | Public |
definition=Open top single deck vehicle - A vehicle with partial roof or without roof. order=21
cj | Public |
definition=Open top double deck vehicle - A vehicle without roof over all or part of its upper deck. order=22
cx | Public |
definition=Bus chassis - An incomplete vehicle with just chassis rails or tube assembly, power train, axles, that is intended to be completed with bodywork, customised to the needs of the transport operator. order=23
da | Public |
definition=Semi-trailer-Trailer that is des. and constr. to be coupled to a tractor unit or converter dolly and to impose a subst. vertical load on the towing vehicle or converter dolly. The coupling for a vehicle comb. shall consist of a king pin and a fifth wheel. order=24
db | Public |
definition=Drawbar trailer-Trailer having at least two axles, with at least one is a steered axle:(a)equipped with a towing device which can move vertically (in relation to trailer); (b)that transmits less than 100daN as static vertical load to the towing vehicle. order=25
dc | Public |
definition=Centre-axle trailer- see definition in REGULATION (EU) 2018/858 Annex 1 Part C Ref. 5.3. order=26
de | Public |
definition=Rigid drawbar trailer- see definition in REGULATION (EU) 2018/858 Annex 1 Part C Ref. 5.4. order=27
Tag | Value
definition | Bodywork codes according to REGULATION (EU) 2018/858.
Details:
Property | Value
isFinalSpecialization: | 0