# Classes::ElectricChargingPointStatus

Project: Classes | ElectricChargingPointStatus : Public <<D2Class>> Class
Created: | 22/01/2019 18:17:40
Modified: | 12/02/2026 12:54:52
Project: |
Author: | Freudenstein
Version: | 1.0
Phase: | 1.0
Status: | Proposed
Complexity: | Easy
Difficulty: |
Priority: |
Multiplicity: |
Advanced: |
UUID: | {F97CD478-2180-42ad-BFFD-6F044D8E6E00}
Appears In: | EnergyInfrastructureStatusPublication
Attributes Tagged Values Advanced Other Links
Attribute | Scope | Type
currentChargingPower | Public | Watt
definition=The current power in watts. order=2
currentVoltage | Public | Volt
definition=Currently used voltage. order=1
nextAvailableChargingSlots | Public | DateTime
definition=One or more points of time in the future, at which the charging point will be available (not occupied and not reserved). order=3
remainingChargingTime | Public | Seconds
definition=If known, the approximate remaining charging time for the current vehicle on this refill point can be specified. order=0
Tag | Value
definition | Dynamic information on the status of the charging point.
Details:
Property | Value
isFinalSpecialization: | 0
Object | Type | Connection | Direction | Notes
«D2Class» RefillPointStatus | Class | Generalization | To |