# GnssExtension::PointCoordinatesExtended

Project: GnssExtension | PointCoordinatesExtended : Public <<D2Class>> Class
Created: | 15/08/2011 13:41:19
Modified: | 29/11/2022 17:26:22
Project: |
Author: | JPhM
Version: | 1.0
Phase: | 1.0
Status: | Proposed
Complexity: | Easy
Difficulty: |
Priority: |
Multiplicity: |
Advanced: |
UUID: | {3CB8B6C2-5F2A-4db1-9936-6272470F3262}
Appears In: | GnssExtension
origin: CWA SCUTUM<br/>originalCode: 69 <br/>originalName: Positioning information (coordinates, speed, direction, ….)<br/> Attributes Associations From Tagged Values Advanced Other Links
Attribute | Scope | Type
authenticationStatus | Public | Boolean
definition=Status of the process performed by the “Authentication Function” ('False" = No Error; "True" = Error occurred - do not use the result) (see WA 16390:2018 Table 9). order=1
Notes: | Status of the processing performed by the “Authentication Function”:<br/> 0 - No Error<br/> 1 - Error occured -do not use the result<br/><br/>If this status reports an error, then authentication result is not needed.<br/><br/>It the status is No Error, then authenticationResult is needed to know on which constellation the authentication is based. <br/>origin: Issued from CWA 16390 Revision<br/><br/>
dateTimeGivenByReceiver | Public | DateTime
definition=This Date/Time is given by the receiver according to the calculated position. order=2
hpl | Public | MetresAsFloat
definition=The horizontal protection level is the radius of a circle centred on the actual position and defining the area in which the calculated position is located with a given degree of confidence. order=3
Notes: | Horizontal Protection Level (HPL). <br/>The horizontal protection level is a circle centred on the actual position with a radius corresponding to the area in which the calculated position is located with a given degree of confidence. This circle is tangent to the reference earth ellipsoid.<br/>This radius is based on the error estimations provided by the GNSS augmentation system (SBAS).<br/>This hpl combined with the vpl (vertical protection level) forms a cylinder in which the calculated position must be located. If not, then it is an integrity error.<br/>
sbasCorrectionApplied | Public | SbasCorrectionEnum
definition=Indicates which corrections according to SBAS are applied. order=4
Notes: | Indicates that correction according to SBAS are applied:<br/> 0 - EGNOS Corrections to GPS Not Applied<br/> 1 - EGNOS Corrections Applied to GPS by Terminal<br/> 2 - EGNOS Corrections Applied to GPS by Service centre<br/><br/>origin: Issued from CWA 16390 Revision (Galileo Navigation Authentication Specification for Signal-In-Space Testing V1.0)<br/><br/><br/>
signature | Public | String
definition=Identification of the organisation that provides the calculation of the position (it can sign it to ensure its identification and non-repudiation to guaranty the final user that it can trust this value). order=5
Notes: | The organisation which provides the calculation of the position can sign it to ensure its identification and non-repudiation to guaranty the final user that it can trust this value. <br/>origin: Issued from GeotransMD project<br/>
srsName | Public | String
definition=Specifies the Coordinate Reference System (CRS) used to interpret the point coordinates.(by default: ETR89-LatLonh). order=0 schemaAttribute=yes
Element | Source Role | Target Role
«D2Class» RawDataMessage Class «D2Relation» | Name: | Name:
Details:
Tag | Value
definition | Additional information provided by means of EGNOS CS and EDAS based services
Details:
Property | Value
isFinalSpecialization: | 0
Object | Type | Connection | Direction | Notes
«D2Class» PointCoordinates | Class | Generalization | To |
«D2Class» RawDataMessage | Class | Strong | From |