# Enumerations::ConnectorTypeEnum

Project: Enumerations | ConnectorTypeEnum : Public <<D2Enumeration>> Enumeration
Created: | 06/09/2017 11:40:22
Modified: | 29/11/2022 17:26:03
Project: |
Author: | Strohschein
Version: | 1.0
Phase: | 1.0
Status: | Proposed
Complexity: | Easy
Difficulty: |
Priority: |
Multiplicity: |
Advanced: |
UUID: | {42F80F68-C2B5-4e33-9A70-95D6EB99659E}
Appears In: | ElectricChargingPoint, EnergyInfrastructureTablePublication
Attributes Tagged Values Advanced
Attribute | Scope | Type
cee3 | Public |
changed=new definition=CEE3, 230 V, 16 A order=8 origin=- null - originalCode=- null - originalName=- null -
cee5 | Public |
changed=new definition=CEE5, 400 V, 16-63 A order=9 origin=- null - originalCode=- null - originalName=- null -
chademo | Public |
changed=new definition=CHAdeMO, 600 V DC. Used mostly in Japan. order=5 origin=- null - originalCode=- null - originalName=- null -
yazaki | Public |
changed=new definition=Yazaki, 400 VDC, 125 A, Asian standard. order=10 origin=- null - originalCode=- null - originalName=- null -
domestic | Public |
definition=A domestic socket of unspecified type. Applicable countries should be specified in separate attribute. order=11
domesticA | Public |
definition=Domestic socket type A (mainly used in the USA, Canada, Mexico & Japan) order=12
domesticB | Public |
definition=Domestic socket type B (mainly used in the USA, Canada & Mexico) order=13
domesticC | Public |
definition=Domestic socket type C (commonly used in Europe, South America & Asia) order=14
domesticD | Public |
definition=Domestic socket type D (mainly used in India) order=15
domesticE | Public |
definition=Domestic socket type E (primarily used in France, Belgium, Poland, Slovakia & Czechia) order=16
domesticF | Public |
definition=Domestic socket type F (used almost everywhere in Europe & Russia, except for the UK & Ireland) order=17
domesticG | Public |
definition=Domestic socket type G (mainly used in the United Kingdom, Ireland, Malta, Malaysia, Singapore & the Arabian Peninsula) order=18
domesticH | Public |
definition=Domestic socket type H (used exclusively in Israel, the West Bank & the Gaza Strip) order=19
domesticI | Public |
definition=Domestic socket type I (mainly used in Australia, New Zealand, China & Argentina) order=20
domesticJ | Public |
definition=Domestic socket type J (used almost exclusively in Switzerland & Liechtenstein) order=21
domesticK | Public |
definition=Domestic socket type K (used almost exclusively in Denmark & Greenland) order=22
domesticL | Public |
definition=Domestic socket type L (used almost exclusively in Italy & Chile) order=23
domesticM | Public |
definition=Domestic socket type M (mainly used in South Africa) order=24
domesticN | Public |
definition=Domestic socket type N (used in Brazil and South Africa) order=25
domesticO | Public |
definition=Domestic socket type O (used exclusively in Thailand) order=26
iec60309x2three16 | Public |
definition=IEC 60309-2 Industrial Connector three phase 16 amperes (usually red) order=31
iec60309x2three32 | Public |
definition=IEC 60309-2 Industrial Connector three phase 32 amperes (usually red) order=32
iec60309x2three64 | Public |
definition=IEC 60309-2 Industrial Connector three phase 64 amperes (usually red) order=33
iec60309x2single16 | Public |
definition= IEC 60309-2 Industrial Connector single phase 16 amperes (usually blue) order=30
iec62196T1 | Public |
definition=IEC 62196 Type 1 "SAE J1772". Mostly used in USA and Asia. order=34
iec62196T1COMBO | Public |
definition=Combo Type 1 based, DC order=35
iec62196T2 | Public |
definition=IEC 62196 Type 2 "Mennekes" - 400 V, 16-63 A. Mandatory in Europe; EN 17186 identifier "C" order=36
iec62196T2COMBO | Public |
definition=Combo Type 2 based, DC, Type 2 connector with extension for simultaneous DC-charging order=37
iec62196T3A | Public |
definition=IEC 62196 Type 3A; EN 17186 identifier "D" order=38
iec62196T3C | Public |
definition= IEC 62196 Type 3C "Scame"; EN 17186 identifier "E" order=39
pantographBottomUp | Public |
definition=On-board Bottom-up-Pantograph typically for bus charging order=40
pantographTopDown | Public |
definition=Off-board Top-down-Pantograph typically for bus charging order=41
teslaConnectorEurope | Public |
changed=new definition=Tesla Connector EU (modification of the Type 2 connector) order=42 origin=- null - originalCode=- null - originalName=- null -
teslaConnectorAmerica | Public |
definition=Tesla connector used in America (Tesla specific) order=43
teslaR | Public |
definition=Tesla Connector "Roadster"-type (round, 4 pin) order=44
teslaS | Public |
definition=Tesla Connector "Model-S"-type (oval, 5 pin) order=45
other | Public |
definition=Other charging interface. order=99
Tag | Value
| List of connector interface types
Details:
changed | new
Details: Default: new
definition | A table of commonly used connectors / charging interfaces
Details:
origin | - null -
Details: Default: - null -
originalCode | - null -
Details: Default: - null -
originalName | - null -
Details: Default: - null -
Property | Value
isFinalSpecialization: | 0