# AlertC::AlertCLinear

Project: AlertC | AlertCLinear : Public abstract <<D2Class>> Class
Created: | 19/11/2004 09:42:50
Modified: | 29/11/2022 17:26:00
Project: |
Author: |
Version: | 1.0
Phase: | 1.0
Status: | Proposed
Complexity: | Easy
Difficulty: |
Priority: |
Multiplicity: |
Advanced: |
UUID: | {538DA6A1-280C-4b5f-8FFA-1CEDF0BA19C2}
Appears In: | LinearLocation
Attributes Associations To Tagged Values Advanced Other Links
Attribute | Scope | Type
alertCLocationCountryCode | Public | String
definition=ALERT-C country code as defined in IEC 62106. order=0
alertCLocationTableNumber | Public | String
definition=Number allocated to an ALERT-C table in a country. Ref. EN ISO 14819-3 for the allocation of a location table number. order=1
alertCLocationTableVersion | Public | String
definition=Version number associated with an ALERT-C table reference. order=2
Element | Source Role | Target Role
«D2Class» SingleRoadLinearLocation Class «D2Relation» | Name: | Name:
Details:
Tag | Value
definition | A linear section along a road defined between two points on the road by reference to a pre-defined ALERT-C location table.
Details:
Property | Value
isFinalSpecialization: | 0
Object | Type | Connection | Direction | Notes
«D2Class» AlertCLinearByCode | Class | Generalization | From |
«D2Class» SingleRoadLinearLocation | Class | Strong | To |
«D2Class» AlertCMethod4Linear | Class | Generalization | From |
«D2Class» AlertCMethod2Linear | Class | Generalization | From |