# AlertC::AlertCMethod4SecondaryPointLocation

Project: AlertC | AlertCMethod4SecondaryPointLocation : Public <<D2Class>> Class
Created: | 10/06/2005 12:41:54
Modified: | 29/11/2022 17:26:01
Project: |
Author: |
Version: | 1.0
Phase: | 1.0
Status: | Proposed
Complexity: | Easy
Difficulty: |
Priority: |
Multiplicity: |
Advanced: |
UUID: | {CBAE58F4-DF40-412b-89C9-A74F0E3A77E6}
Appears In: | AlertCMethod4Linear
Associations To Associations From Tagged Values Advanced Other Links
Element | Source Role | Target Role
«D2Class» AlertCMethod4Linear Class «D2Relation» | Name: | Name:
Details:
Element | Source Role | Target Role
«D2Class» AlertCLocation Class «D2Relation» | Name: | Name:
Details:
«D2Class» OffsetDistance Class «D2Relation» | Name: | Name:
Details:
Tag | Value
definition | The point (called Secondary point) which is at the upstream end of a linear road section. The point is specified by a reference to a point in a pre-defined Alert-C location table plus a non-negative offset distance.
Details:
Property | Value
isFinalSpecialization: | 0
Object | Type | Connection | Direction | Notes
«D2Class» AlertCLocation | Class | Strong | From |
«D2Class» OffsetDistance | Class | Strong | From |
«D2Class» AlertCMethod4Linear | Class | Strong | To |