# Enumerations::ConnectorFormatTypeEnum

Project: Enumerations | ConnectorFormatTypeEnum : Public <<D2Enumeration>> Enumeration
Created: | 13/06/2019 09:52:16
Modified: | 12/02/2026 12:54:52
Project: |
Author: | Strohschein
Version: | 1.0
Phase: | 1.0
Status: | Proposed
Complexity: | Easy
Difficulty: |
Priority: |
Multiplicity: |
Advanced: |
UUID: | {87531E3B-1C6E-45ec-AA9A-FBB70A74925D}
Appears In: | ElectricChargingPoint, EnergyInfrastructureTablePublication
Attributes Tagged Values Advanced
Attribute | Scope | Type
cableMode2 | Public |
definition=The connector is an attached cable; the EV users car needs to have a fitting inlet for a mode 2 cable, common for most domestic sockets. order=0
cableMode3 | Public |
definition=The connector is an attached cable; the EV users car needs to have a fitting inlet for a mode 3 cable, can be used for Type 1 and Type 2 sockets. order=1
otherCable | Public |
definition=The connector is an attached cable; the EV users car needs to have a fitting inlet. order=2
socket | Public |
definition=The connector is a socket; the EV user needs to bring a fitting plug. order=3
Tag | Value
definition | A list of cable types used during the charging process.
Details:
Property | Value
isFinalSpecialization: | 0