# Classes::Connector

Project: Classes | Connector : Public <<D2Class>> Class
Created: | 03/08/2017 11:01:15
Modified: | 12/02/2026 12:54:52
Project: |
Author: | Strohschein
Version: | 1.0
Phase: | 1.0
Status: | Proposed
Complexity: | Easy
Difficulty: |
Priority: |
Multiplicity: |
Advanced: |
UUID: | {2B8F4B3A-D2E0-4550-BC1B-94B07100597F}
Appears In: | ElectricChargingPoint, EnergyInfrastructureTablePublication
Attributes Associations To Associations From Tagged Values Advanced Other Links
Attribute | Scope | Type
connectorFormat | Public | ConnectorFormatTypeEnum
definition=Information on the cable type used. order=5
connectorType | Public | ConnectorTypeEnum
changed=new definition=Specification of the connector, i.e. the charging interface type. order=1 origin=- null - originalCode=- null - originalName=- null -
countryOfDomesticSocket | Public | CountryCode
definition=Countries for which the domestic socket is applicable. Only needed if explicit type of a domestic socket is not specified. order=3
maximumCurrent | Public | Ampere
definition=Maximum current in ampere. order=8
maxPowerAtSocket | Public | Watt
changed=new definition=Maximum power at the socket in watts. order=6 origin=- null - originalCode=- null - originalName=- null -
otherConnector | Public | String
definition=Some other connector / charging interface. order=2
voltage | Public | Volt
definition=Voltage at the connector. order=7
Element | Source Role | Target Role
«D2Class» ElectricChargingPoint Class «D2Relation» | Name: | Name:
Details:
Element | Source Role | Target Role
«D2Class» ExternalIdentifier Class «D2Relation» | Name: | Name:
Details:
Tag | Value
changed | new
Details: Default: new
definition | Parameters and description of an interface that is available at the given electric charging point to connect vehicles.
Details:
Property | Value
isFinalSpecialization: | 0
Object | Type | Connection | Direction | Notes
«D2Class» ExternalIdentifier | Class | Strong | From |
«D2Class» ElectricChargingPoint | Class | Strong | To |