# VmsMessage::VmsMessage

Project: VmsMessage | VmsMessage : Public <<D2Class>> Class
Created: | 26/02/2020 22:50:26
Modified: | 29/11/2022 17:26:13
Project: |
Author: |
Version: | 1.0
Phase: | 1.0
Status: | Proposed
Complexity: | Easy
Difficulty: |
Priority: |
Multiplicity: |
Advanced: |
UUID: | {F926BF87-C704-4afc-9390-239F5478B046}
Appears In: | VmsMessage, VmsStatus
Attributes Associations To Associations From Tagged Values Advanced Other Links
Attribute | Scope | Type
associatedTrafficManagementPlan | Public | String
definition=The identification of the traffic management plan or diversion plan with which the message is associated. order=0
codedReasonForSetting | Public | SettingReasonEnum
definition=The reason, in terms of a high-level coded classification, why the sign has been set. order=4
distanceFromClosestSituationRecord | Public | MetresAsFloat
definition=Distance of the VMS from the location of the closest situation record. If the VMS is located within the extent of the situation record this should be set to zero. order=12
mareNostrumCompliant | Public | Boolean
definition=Indication that the displayed message (text and pictogram) conforms with the formulation recommended by the Mare Nostrum project. order=7
messageInformationType | Public | MessageInformationTypeEnum
definition=Type of information being displayed. order=5
messageSetBy | Public | MultilingualString
definition=The organisation or authority which set the message currently being displayed. order=1
primarySetting | Public | Boolean
definition=Identifies whether the message setting is primary (explicitly requested) or is secondary (derived according to an algorithm as the result of setting other signs). True = a primary setting. order=6
reasonForSetting | Public | MultilingualString
definition=The reason why the sign has been set. order=3
relatedSituation | Public | VersionedReference
definition=A reference to the managed situation to which the set message relates. order=10 targetClass=sit:Situation
relatedSituationRecord | Public | VersionedReference
definition=A reference to the situation record within a managed situation to which the set message relates. order=11 targetClass=sit:SituationRecord
requestedBy | Public | MultilingualString
definition=The authority, organisation or system which requested the setting of the message. This may be different from the authority or system which actually set the message on behalf of the requestor. order=9
sequencingInterval | Public | Seconds
definition=The time duration that each text page or pictogram within a message is displayed for before the VMS displays the next text page and/or pictogram in the message. order=13
setBySystem | Public | Boolean
definition=Indicates whether the message has been set automatically by a system. True = automatically set. order=2
timeLastSet | Public | DateTime
definition=The date/time at which the sign was last set. order=8
Element | Source Role | Target Role
«D2Class» VmsStatus Class «D2Relation» | Name: | Name:
Details:
Element | Source Role | Target Role
«D2Class» Image Class «D2Relation» | Name: | Name:
Details:
«D2Class» DisplayAreaSettings Class «D2Relation» | Name: | Name:
Details:
Tag | Value
definition | A message displayed on a VMS which can comprise one or more sequentially displayed text pages and/or pictograms with supplementary details.
Details:
Property | Value
isFinalSpecialization: | 0
Object | Type | Connection | Direction | Notes
«D2Class» Image | Class | Strong | From |
«D2Class» DisplayAreaSettings | Class | Strong | From |
«D2Class» VmsStatus | Class | Strong | To |