# Enumerations::InfrastructureDamageTypeEnum

Project: Enumerations | InfrastructureDamageTypeEnum : Public <<D2Enumeration>> Enumeration
Created: | 17/06/2004 16:52:25
Modified: | 29/11/2022 17:26:10
Project: |
Author: |
Version: | 1.0
Phase: | 1.0
Status: | Proposed
Complexity: | Easy
Difficulty: |
Priority: |
Multiplicity: |
Advanced: |
UUID: | {CB4CE3F6-900F-4724-A212-3B072403A478}
Appears In: | Enumerations, InfrastructureDamageType
Attributes Tagged Values Advanced Other Links
Attribute | Scope | Type
burstPipe | Public | enumerationLiteral
definition=The road surface has sunken or collapsed in places due to burst pipes. order=0
burstWaterMain | Public | enumerationLiteral
definition=Traffic may be disrupted due to local flooding and/or subsidence because of a broken water main. order=1
collapsedSewer | Public | enumerationLiteral
definition=The road surface has sunken or collapsed in places due to sewer failure. order=2
damagedBridge | Public | enumerationLiteral
definition=Damage to a bridge that may cause traffic disruption. order=3
damagedCrashBarrier | Public | enumerationLiteral
definition=Damage to a crash barrier that may cause traffic disruption. order=4
damagedFlyover | Public | enumerationLiteral
definition=Damage to an elevated section of the carriageway over another carriageway that may cause traffic disruption. order=5
damagedGallery | Public | enumerationLiteral
definition=Damage to a gallery that may cause traffic disruption. order=6
damagedGantry | Public | enumerationLiteral
definition=Damage to a gantry above the roadway that may cause traffic disruption. order=7
damagedRoadSurface | Public | enumerationLiteral
definition=Damage to the road surface that may cause traffic disruption. order=8
damagedTunnel | Public | enumerationLiteral
definition=Damage to a tunnel that may cause traffic disruption. order=9
damagedViaduct | Public | enumerationLiteral
definition=Damage to a viaduct that may cause traffic disruption. order=10
fallenPowerCables | Public | enumerationLiteral
definition=The road is obstructed or partially obstructed by one or more fallen power cables. order=11
gasLeak | Public | enumerationLiteral
definition=Traffic may be disrupted due to an explosion hazard from gas escaping in or near the roadway. order=12
weakBridge | Public | enumerationLiteral
definition=Weak bridge capable of carrying a reduced load, typically with a reduced weight limit restriction imposed. order=13
other | Public | enumerationLiteral
definition=Other than as defined in this enumeration. order=14
Tag | Value
definition | Types of infrastructure damage which may have an effect on the road network.
Details:
Property | Value
isFinalSpecialization: | 0
Object | Type | Connection | Direction | Notes
«D2Enumeration» InfrastructureDamageTypeEnumExtendedUrban | Enumeration | Generalization | From |