# Enumerations::FaultSeverityEnum

Project: Enumerations | FaultSeverityEnum : Public <<D2Enumeration>> Enumeration
Created: | 22/03/2010 10:18:14
Modified: | 29/11/2022 17:25:58
Project: |
Author: |
Version: | 1.0
Phase: | 1.0
Status: | Proposed
Complexity: | Easy
Difficulty: |
Priority: |
Multiplicity: |
Advanced: |
UUID: | {D6F6234E-0625-4292-9297-FF835D60CD4A}
Appears In: | Enumerations
Attributes Tagged Values Advanced
Attribute | Scope | Type
low | Public | enumerationLiteral
definition=The fault is of low severity and has only limited impact on the usability of the equipment or the value of the data generated by the equipment. order=0
medium | Public | enumerationLiteral
definition=The fault is of medium severity which will significantly limit the usability of the equipment or devalue the usefulness of the data generated by the equipment. order=1
high | Public | enumerationLiteral
definition=The fault is of high severity which will render the equipment unusable or any data generated by the equipment to be of no value. order=2
unknown | Public | enumerationLiteral
definition=The fault is of unknown severity and hence its effect on the usability of the equipment or the usefulness of the data generated by the equipment can not be assessed. order=3
Tag | Value
definition | Classification of the severity of faults.
Details:
Property | Value
isFinalSpecialization: | 0