# SupplementaryPositionalDescription::SupplementaryPositionalDescription

Project: SupplementaryPositionalDescription | SupplementaryPositionalDescription : Public <<D2Class>> Class
Created: | 26/08/2004 08:22:51
Modified: | 29/11/2022 17:26:01
Project: |
Author: |
Version: | 1.0
Phase: | 1.0
Status: | Proposed
Complexity: | Easy
Difficulty: |
Priority: |
Multiplicity: |
Advanced: |
UUID: | {EB0BF15E-C269-4f69-86DC-94F1518CB8CC}
Appears In: | LocationReference, LinearLocation, SupplementaryPositionalDescription, LocationExtension (stable elements), ReroutingManagement, ReroutingManagement Complete wide, ReroutingManagement Structure
Attributes Associations To Associations From Tagged Values Advanced Other Links
Attribute | Scope | Type
directionPurpose | Public | DirectionPurposeEnum
definition=Identifies the main purpose of the road at the location order=0
geographicDescriptor | Public | GeographicCharacteristicEnum
definition=Descriptor which identifies a geographic characteristic to help identify the specific location order=1
infrastructureDescriptor | Public | InfrastructureDescriptorEnum
definition=Descriptor which identifies infrastructure to help identify the specific location. order=2
lengthAffected | Public | MetresAsFloat
definition=This indicates the length (measured in metres) of carriageway (and lanes) affected by the associated traffic element. order=3
locationDescription | Public | MultilingualString
definition=Supplementary human-readable description of the location order=4
locationPrecision | Public | MetresAsNonNegativeInteger
definition=Indicates that the location is given with a precision which is better than the stated value in metres. order=5 schemaAttribute=yes
positionOnCarriageway | Public | RelativePositionOnCarriagewayEnum
definition=Relative position across carriageway order=6
sequentialRampNumber | Public | NonNegativeInteger
definition=The sequential number of an exit/entrance ramp from a given location in a given direction (normally used to indicate a specific exit/entrance in a complex junction/intersection). order=7
Element | Source Role | Target Role
«D2Class» NetworkLocation Class «D2Relation» | Name: | Name:
Details:
«D2Class» RouteDescription Class «D2Relation» | Name: | Name:
Details:
«D2Class» LinearLocation Class «D2Relation» | Name: secondarySupplementaryDescription | Name:
Details:
Element | Source Role | Target Role
«D2Class» NamedArea Class «D2Relation» | Name: | Name:
Details:
«D2Class» RoadInformation Class «D2Relation» | Name: | Name:
Details:
«D2Class» Carriageway Class «D2Relation» | Name: | Name:
Details:
Tag | Value
definition | A collection of supplementary positional information which improves the precision of the location.
Details:
Property | Value
isFinalSpecialization: | 0
Object | Type | Connection | Direction | Notes
«D2Class» NamedArea | Class | Strong | From |
«D2Class» SupplementaryPositionalDescriptionExtended | Class | Generalization | From |
«D2Class» NetworkLocation | Class | Strong | To |
«D2Class» RoadInformation | Class | Strong | From |
«D2Class» RouteDescription | Class | Strong | To |
«D2Class» LinearLocation | Class | Strong | To |
«D2Class» Carriageway | Class | Strong | From |