# Enumerations::WeatherRelatedRoadConditionTypeEnum

Project: Enumerations | WeatherRelatedRoadConditionTypeEnum : Public <<D2Enumeration>> Enumeration
Created: | 17/06/2004 19:31:56
Modified: | 29/11/2022 17:25:59
Project: |
Author: |
Version: | 1.0
Phase: | 1.0
Status: | Proposed
Complexity: | Easy
Difficulty: |
Priority: |
Multiplicity: |
Advanced: |
UUID: | {6B1CA617-8B38-4b04-A8F6-E7BFF5BFBDD4}
Appears In: | Enumerations
Attributes Tagged Values Advanced
Attribute | Scope | Type
blackIce | Public | enumerationLiteral
definition=Severe skid risk due to black ice (i.e. clear ice, which is impossible or very difficult to see). order=0
deepSnow | Public | enumerationLiteral
definition=Deep snow on the roadway. order=1
dry | Public | enumerationLiteral
definition=There is no humidity over the sensor. order=2
freezingOfWetRoads | Public | enumerationLiteral
definition=The wet road surface is subject to freezing. order=3
freezingPavements | Public | enumerationLiteral
definition=The pavements for pedestrians are subject to freezing. order=4
freezingRain | Public | enumerationLiteral
definition=Severe skid risk due to rain falling on sub-zero temperature road surface and freezing. order=5
freshSnow | Public | enumerationLiteral
definition=Fresh snow (with little or no traffic yet) on the roadway. order=6
glaze | Public | enumerationLiteral
definition=Glaze of the road surface. order=7
ice | Public | enumerationLiteral
definition=Increased skid risk due to ice (of any kind). order=8
iceBuildUp | Public | enumerationLiteral
definition=Ice is building up on the roadway causing a serious skid hazard. order=9
iceWithWheelBarTracks | Public | enumerationLiteral
definition=Ice on the road frozen in the form of wheel tracks. order=11
icyPatches | Public | enumerationLiteral
definition=Severe skid risk due to icy patches (i.e. intermittent ice on roadway). order=12
looseSnow | Public | enumerationLiteral
definition=Powdery snow on the road which is subject to being blown by the wind. order=13
moist | Public | enumerationLiteral
definition=From (0,01 mm) water film thickness over the sensor order=14
normalWinterConditionsForPedestrians | Public | enumerationLiteral
definition=Conditions for pedestrians are consistent with those normally expected in winter. order=15
notDry | Public | enumerationLiteral
definition=The road surface is not dry. order=16
packedSnow | Public | enumerationLiteral
definition=Packed snow (heavily trafficked) on the roadway. order=17
rime | Public | enumerationLiteral
definition=Fresh snow (with little or no traffic yet) on the roadway. order=18
roadSurfaceMelting | Public | enumerationLiteral
definition=The road surface is melting, or has melted due to abnormally high temperatures. order=19
slippery | Public | enumerationLiteral
definition=Detection at least of the presence of partly or wholly solidified aqueous solution over the sensor. order=20
slushOnRoad | Public | enumerationLiteral
definition=Increased skid risk due to melting snow (slush) on road. order=21
slushStrings | Public | enumerationLiteral
definition=Melting snow (slush) on the roadway is formed into wheel tracks. order=22
snow | Public | enumerationLiteral
definition=Fresh snow (with little or no traffic yet) on the roadway. order=23
snowDrifts | Public | enumerationLiteral
definition=Snow drifting is in progress or patches of deep snow are present due to earlier drifting. order=24
snowOnPavement | Public | enumerationLiteral
definition=Snow is on the pedestrian pavement. order=25
wetAndIcyRoad | Public | enumerationLiteral
definition=Increased skid risk due to partly thawed, wet road with packed snow and ice, or rain falling on packed snow and ice. order=26
snowOnTheRoad | Public | enumerationLiteral
definition=Snow is lying on the road surface. order=27
wetIcyPavement | Public | enumerationLiteral
definition=Partly thawed, wet pedestrian pavement with packed snow and ice, or rain falling on packed snow and ice. order=28
streamingWater | Public | enumerationLiteral
definition=From (2 mm) water film thickness over the sensor. order=29
surfaceWater | Public | enumerationLiteral
definition=Water is resting on the roadway which provides an increased hazard to vehicles. order=30
wet | Public | enumerationLiteral
definition=From (0,2 mm) water film thickness over the sensor order=31
other | Public | enumerationLiteral
definition=Other than as defined in this enumeration. order=99
Tag | Value
definition | Types of road surface conditions which are related to the weather.
Details:
Property | Value
isFinalSpecialization: | 0