# GnssExtension::RawDataMessage

Project: GnssExtension | RawDataMessage : Public <<D2Class>> Class
Created: | 31/05/2011 09:57:23
Modified: | 29/11/2022 17:26:22
Project: |
Author: | JPhMechin
Version: | 1.0
Phase: | 1.0
Status: | Proposed
Complexity: | Easy
Difficulty: |
Priority: |
Multiplicity: |
Advanced: |
UUID: | {1BFDD5DC-1036-453e-887F-9EF0DE4EBC10}
Appears In: | GnssExtension
origin: CWA SCUTUM<br/> Attributes Associations To Associations From Tagged Values Advanced Other Links
Attribute | Scope | Type
extendedGpsWeekNumber | Public | NonNegativeInteger
definition=Extended GNSS week number (integer number of weeks without roll-over) order=0
Notes: | origin: CWA 16390:2018<br/>
gpsTimeOfWeek | Public | NonNegativeInteger
definition= GPS time of week i.e.the number of milliseconds elapsed since the beginning of the considered week. order=1
Notes: | Milliseconds<br/>According to CWA 16390 Revision, all the measurements shall be referred to a single coordinate/time system in order to avoid ambiguities and to enable a proper interoperability.<br/><br/>Two fields are used to specify GPS time of measurement, following the convention below:<br/><ul> <li>GPS time of week (milliseconds)</li></ul> <ul> <li>Extended GPS week number (integer number of weeks without roll-over).</li></ul><p/>
x | Public | MetresAsFloat
definition=X coordinate in Earth-centred, Earth-fixed (ECEF) Cartesian coordinate system (Origin = Earth’s centre of mass). order=2
Notes: | WGS84 ECEF coordinate system<br/>
y | Public | MetresAsFloat
definition=Y coordinate in Earth-centred, Earth-fixed (ECEF) Cartesian coordinate system (Origin = Earth’s centre of mass). order=3
Notes: | WGS84 ECEF coordinate system<br/>
z | Public | MetresAsFloat
definition=Z coordinate in Earth-centred, Earth-fixed (ECEF) Cartesian coordinate system (Origin = Earth’s centre of mass). order=4
Notes: | WGS84 ECEF coordinate system<br/>
Element | Source Role | Target Role
«D2Class» PointCoordinatesExtended Class «D2Relation» | Name: | Name:
Details:
Element | Source Role | Target Role
«D2Class» SbasCorrectionAndAuthenticationPerConstellation Class «D2Relation» | Name: | Name:
Details:
«D2Class» TrackedSatellite Class «D2Relation» | Name: | Name:
Details:
Tag | Value
definition | Message containing raw data from the receiver to the algorithm that calculates position
Details:
Property | Value
isFinalSpecialization: | 0
Object | Type | Connection | Direction | Notes
«D2Class» SbasCorrectionAndAuthenticationPerConstellation | Class | Strong | From |
«D2Class» PointCoordinatesExtended | Class | Strong | To |
«D2Class» TrackedSatellite | Class | Strong | From |