# GnssExtension::HeightCoordinateExtended

Project: GnssExtension | HeightCoordinateExtended : Public <<D2Class>> Class
Created: | 16/06/2020 09:55:25
Modified: | 29/11/2022 17:26:21
Project: |
Author: | jean-philippe.mechin
Version: | 1.0
Phase: | 1.0
Status: | Proposed
Complexity: | Easy
Difficulty: |
Priority: |
Multiplicity: |
Advanced: |
UUID: | {8B4003F2-69FB-4b5a-A4BC-2D03466E081D}
Appears In: | GnssExtension
Attributes Tagged Values Advanced Other Links
Attribute | Scope | Type
vpl | Public | MetresAsFloat
definition=The vertical protection level is the half-length of the vertical segment on either side of the actual position that defines the zone in which the calculated position is located with a given degree of confidence. order=0
Tag | Value
definition | Height coordinate extended to provide the Vertical Protection Level which is calculated according to the GNSS rules.
Details:
Property | Value
isFinalSpecialization: | 0
Object | Type | Connection | Direction | Notes
«D2Class» HeightCoordinate | Class | Generalization | To |