# Enumerations::RoadOrCarriagewayOrLaneManagementTypeEnum

Project: Enumerations | RoadOrCarriagewayOrLaneManagementTypeEnum : Public <<D2Enumeration>> Enumeration
Created: | 25/08/2004 07:31:27
Modified: | 29/11/2022 17:26:12
Project: |
Author: |
Version: | 1.0
Phase: | 1.0
Status: | Proposed
Complexity: | Easy
Difficulty: |
Priority: |
Multiplicity: |
Advanced: |
UUID: | {C76C4E19-C7D9-4938-8BA5-8B5CDD35137A}
Appears In: | Enumerations, UrbanExtensions, RoadOrCarriagewayOrLaneManagement, SituationExtension
Attributes Tagged Values Advanced Other Links
Attribute | Scope | Type
carPoolLaneInOperation | Public | enumerationLiteral
definition=Dedicated car pool lane(s) are in operation for vehicles carrying at least the specified number of occupants. order=0
carriagewayClosures | Public | enumerationLiteral
definition=Carriageway closures are in operation at the specified location. order=1
clearALaneForEmergencyVehicles | Public | enumerationLiteral
definition=Clear a lane for emergency vehicles. order=2
clearALaneForSnowploughsAndGrittingVehicles | Public | enumerationLiteral
definition=Clear a lane for snow ploughs and gritting vehicles. order=3
closedPermanentlyForTheWinter | Public | enumerationLiteral
definition=The road is closed to vehicles with the specified characteristics or all, if none defined, for the duration of the winter. order=4
contraflow | Public | enumerationLiteral
definition=Two-way traffic is temporarily sharing a single carriageway. order=5
doNotUseSpecifiedLanesOrCarriageways | Public | enumerationLiteral
definition=Do not use the specified lane(s) or carriageway(s). order=6
hardShoulderRunningInOperation | Public | enumerationLiteral
definition=The hard shoulder is open as an operational lane. order=7
hardShoulderRunningNotInOperation | Public | int
definition=the hardshoulder used for dynamic hardshoulder management is closed to vehicles i.e. not running order=8
heightRestrictionInOperation | Public | enumerationLiteral
definition=A height restriction is in operation. order=9
intermittentShortTermClosures | Public | enumerationLiteral
definition=Road closures occur intermittently on the specified road in the specified direction for short durations. order=10
keepToTheLeft | Public | enumerationLiteral
definition=Keep to the left. order=11
keepToTheRight | Public | enumerationLiteral
definition=Keep to the right. order=12
laneClosures | Public | enumerationLiteral
definition=Lane closures are in operation at the specified location for vehicles with the specified characteristics or all, if none defined, in the specified direction. order=13
lanesDeviated | Public | enumerationLiteral
definition=Lane deviations are in operation at the specified location. order=14
narrowLanes | Public | enumerationLiteral
definition=Normal lane widths are temporarily reduced. order=15
newRoadworksLayout | Public | enumerationLiteral
definition=A new layout of lanes/carriageway has been implemented associated with roadworks. order=16
overnightClosures | Public | enumerationLiteral
definition=Every night the road is closed to vehicles with the specified characteristics or all, if none defined, in the specified direction by decision of the appropriate authorities. order=17
roadCleared | Public | enumerationLiteral
definition=The road has been cleared of earlier reported problems. order=18
roadClosed | Public | enumerationLiteral
definition=The road is closed to vehicles with the specified characteristics or all, if none defined, in the specified direction. order=19
rollingRoadBlock | Public | enumerationLiteral
definition=Traffic officers or police are driving slowly in front of a queue of traffic to create a gap in the traffic to allow for clearance activities to take place in safety on the road ahead. order=20
rushHourLaneInOperation | Public | enumerationLiteral
definition=Dedicated rush (peak) hour lane(s) are in operation. order=21
singleAlternateLineTraffic | Public | enumerationLiteral
definition=Traffic is being controlled to move in alternate single lines. This control may be undertaken by traffic lights or flagman. order=22
tidalFlowLaneInOperation | Public | enumerationLiteral
definition=Dedicated tidal flow lane(s) are in operation in the specified direction. order=23
turnAroundInOperation | Public | enumerationLiteral
definition=Traffic is being directed back down the opposite carriageway, possibly requiring the temporary removal of the central crash barrier. order=24
useOfSpecifiedLanesOrCarriagewaysAllowed | Public | enumerationLiteral
definition=The specified lane(s) or carriageway(s) may be used. The normal lane(s) or carriageway(s) restrictions are not currently in force. order=25
useSpecifiedLanesOrCarriageways | Public | enumerationLiteral
definition=Use the specified lane(s) or carriageway(s). order=26
vehicleStorageInOperation | Public | enumerationLiteral
definition=Vehicles are being stored on the roadway and/or at a rest area or service area at the specified location. order=27
weightRestrictionInOperation | Public | enumerationLiteral
definition=A weight restriction is in operation. order=28
other | Public | enumerationLiteral
definition=Other than as defined in this enumeration. order=29
Tag | Value
definition | Management actions relating to road, carriageway or lane usage.
Details:
Property | Value
isFinalSpecialization: | 0
Object | Type | Connection | Direction | Notes
«D2Enumeration» RoadOrCarriagewayOrLaneManagementTypeExtended | Enumeration | Generalization | From |
«D2Enumeration» RoadOrCarriageWayOrLaneManagementTypeEnumExtendedUrban | Enumeration | Generalization | From |