# Enumerations::JunctionClassificationEnum

Project: Enumerations | JunctionClassificationEnum : Public <<D2Enumeration>> Enumeration
Created: | 07/09/2011 10:43:17
Modified: | 29/11/2022 17:26:19
Project: |
Author: | Freudenstein
Version: | 1.0
Phase: | 1.0
Status: | Proposed
Complexity: | Easy
Difficulty: |
Priority: |
Multiplicity: |
Advanced: |
UUID: | {8A09433C-4D58-4e33-8B26-9CCC80E28F17}
Appears In: | PointByJunction, AccessRoad
Attributes Tagged Values Advanced
Attribute | Scope | Type
threeWayInterchange | Public | enumerationLiteral
definition=One motorway merging into another (with three legs in total). order=0
interchange | Public | enumerationLiteral
definition=Usually two crossing motorways (four legs, but can be even more). order=1
motorwayConnection | Public | enumerationLiteral
definition=Beginning or end of a motorway (e.g. changeover to smaller road). order=2
junction | Public | enumerationLiteral
definition=Entrance and exit on a motorway. order=3
temporarilyJunction | Public | enumerationLiteral
definition=Entrance and exit on a motorway, reserved either for emergency and service or on a temporarily basis. order=4
borderCrossing | Public | enumerationLiteral
definition=Motorway crossing a border (between counties, countries, states, ...). order=5
junctionInOneDirection | Public | enumerationLiteral
definition=Entry and Exit on a motorway, where just one direction of the motorway is accessible. order=6
operationalServiceJunction | Public | enumerationLiteral
definition=Junction accessible only for operational services. order=7
other | Public | enumerationLiteral
definition=Other. order=99
Tag | Value
definition | Explicit type of a junction.
Details:
Property | Value
isFinalSpecialization: | 0