# Enumerations::ParkingSpaceOccupancyDetectionEnum

Project: Enumerations | ParkingSpaceOccupancyDetectionEnum : Public <<D2Enumeration>> Enumeration
Created: | 22/04/2018 06:25:39
Modified: | 29/11/2022 17:26:20
Project: |
Author: | Jon
Version: | 1.0
Phase: | 1.0
Status: | Proposed
Complexity: | Easy
Difficulty: |
Priority: |
Multiplicity: |
Advanced: |
UUID: | {75FAFEAC-53CD-491e-8D15-9E4AA07882D9}
Appears In: | Space, Enumerations
Attributes Tagged Values Advanced
Attribute | Scope | Type
visual | Public | Enumeration
definition=Operator/owner makes periodic visual counts of the facility. order=1
anpr | Public | Enumeration
definition=Automated License Plate Recognition information is tracked for inbound and outbound traffic. The difference between in and out counts enables an occupancy count. order=2
imageAnalytics | Public | Enumeration
definition=Image analytics are used to evaluate a picture with known parking space geography and computer vision is used to determine occupancy at a point in time. order=3
videoAnalytics | Public | Enumeration
definition=Video analytics are used to evaluate a video stream to identify objects (vehicles) and direction of travel. The difference between the inbound objects and outbound objects determines occupancy. order=4
videoSpace | Public | Enumeration
definition=Video analytics or ANPR technologies are used to evaluate a video stream with known space geometry to identify objects (vehicles or license plates) occupying specific spaces. order=5
spaceSensor | Public | Enumeration
definition=A sensor in each space detects the presence of a vehicle. order=6
userDeclaration | Public | Enumeration
definition=User self-declared, where the user enters a space identifier and/or vehicle registration number, typically at the start of a parking session. order=7
balancing | Public | enumerationLiteral
definition=Counting and balancing incoming and outcoming traffic amount ('indirect' method). order=8
modelBased | Public | enumerationLiteral
definition=Occupancy detection is based on some model, i.e. hydrograph, forecasting or estimation. order=9
none | Public | enumerationLiteral
definition=No occupancy detection available. order=10
unknown | Public | enumerationLiteral
definition=Unknown. order=11
other | Public | enumerationLiteral
definition=Other. order=99
Tag | Value
definition | A list of supported methods for detection of occupancy by a vehicle in a parking space.
Details:
Property | Value
isFinalSpecialization: | 0