# Classes::Connector

Project: Classes | Connector : Public <<D2Class>> Class
Created: | 03/08/2017 11:01:15
Modified: | 29/11/2022 17:26:02
Project: |
Author: | Strohschein
Version: | 1.0
Phase: | 1.0
Status: | Proposed
Complexity: | Easy
Difficulty: |
Priority: |
Multiplicity: |
Advanced: |
UUID: | {E5D9EB2F-7F9D-4a3b-9A7C-9CB63A2DF208}
Appears In: | ElectricChargingPoint, EnergyInfrastructureTablePublication
Attributes Associations To Tagged Values Advanced Other Links
Attribute | Scope | Type
chargingMode | Public | ChargingModeEnum
definition=Available charging modes order=3
connectorFormat | Public | ConnectorFormatTypeEnum
definition=Information on the cable type used. order=4
connectorType | Public | ConnectorTypeEnum
changed=new definition=Specification of the connector, i.e. the charging interface type order=0 origin=- null - originalCode=- null - originalName=- null -
countryOfDomesticSocket | Public | CountryCode
definition=Countries for which the domestic socket is applicable. Only needed if explicit type of a domestic socket is not specified. order=2
maximumCurrent | Public | Ampere
definition=Maximum current in Ampere order=7
maxPowerAtSocket | Public | Watt
changed=new definition=Maximum power at the socket in Watts order=5 origin=- null - originalCode=- null - originalName=- null -
otherConnector | Public | String
definition=Some other connector / charging interface order=1
voltage | Public | Volt
definition=Possible degrees of voltage. order=6
Element | Source Role | Target Role
«D2Class» ElectricChargingPoint Class «D2Relation» | Name: | Name:
Details:
Tag | Value
changed | new
Details: Default: new
definition | Parameters and description of an interface that is available at the given electric charging point to connect vehicles
Details:
Property | Value
isFinalSpecialization: | 0
Object | Type | Connection | Direction | Notes
«D2Class» ElectricChargingPoint | Class | Strong | To |