# OpenLR::OpenlrLineAttributes

Project: OpenLR | OpenlrLineAttributes : Public <<D2Class>> Class
Created: | 18/03/2010 13:32:45
Modified: | 29/11/2022 17:26:02
Project: |
Author: |
Version: | 1.0
Phase: | 1.0
Status: | Proposed
Complexity: | Easy
Difficulty: |
Priority: |
Multiplicity: |
Advanced: |
UUID: | {CBBDB09F-DA46-41df-BFD2-A180A5FD1A1F}
Appears In: | OpenLRPoint
Attributes Associations To Tagged Values Advanced Other Links
Attribute | Scope | Type
openlrBearing | Public | AngleInDegrees
definition=defines the bearing field as an integer value between 0 and 359 order=2
openlrFormOfWay | Public | OpenlrFormOfWayEnum
definition=A classification based on the importance of the role that the Road Element (or Ferry Connection) performs in the connectivity of the total road network. (EN ISO 14825 § 7.2.88) order=1
openlrFunctionalRoadClass | Public | OpenlrFunctionalRoadClassEnum
definition=Certain aspects of the physical form that a Road Element takes. It is based on a number of certain physical and traffic properties. (EN ISO 14825 § 7.2.85) order=0
Element | Source Role | Target Role
«D2Class» OpenlrBaseReferencePoint Class «D2Relation» | Name: | Name:
Details:
Tag | Value
definition | Line attributes are part of a location reference point and consists of functional road class (FRC),form of way (FOW) and bearing (BEAR) data.
Details:
Property | Value
isFinalSpecialization: | 0
Object | Type | Connection | Direction | Notes
«D2Class» OpenlrBaseReferencePoint | Class | Strong | To |