# Enumerations::VmsTypeEnum

Project: Enumerations | VmsTypeEnum : Public <<D2Enumeration>> Enumeration
Created: | 27/02/2020 00:06:53
Modified: | 29/11/2022 17:26:14
Project: |
Author: |
Version: | 1.0
Phase: | 1.0
Status: | Proposed
Complexity: | Easy
Difficulty: |
Priority: |
Multiplicity: |
Advanced: |
UUID: | {173314A0-3B26-4244-AA30-D64A54648E61}
Appears In: | Enumerations
Attributes Tagged Values Advanced
Attribute | Scope | Type
colourGraphic | Public | enumerationLiteral
definition=A colour graphic display. order=0
rotatingPrismSign | Public | enumerationLiteral
definition=A sign implementing fixed messages which are made visible to drivers by electromechanical means e.g. a fixed sign parallel to traffic flow and therefore not legible is rotated to be orthogonal to traffic flow and becomes legible. order=1
monochromeGraphic | Public | enumerationLiteral
definition=A monochrome graphic display. order=2
simpleMatrixSign | Public | enumerationLiteral
definition=Simple display made up of a fixed matrix of pixels (e.g. sets of LEDs or lights) capable of showing a limited set of aspects (or matrix images). The display area is regarded as a pictogram area in DATEX II. order=3
fullMatrixSign | Public | enumerationLiteral
definition=A full-matrix sign. order=4
rollerBlindSign | Public | enumerationLiteral
definition=Continuous sign using a roller blind. order=5
virtualVms | Public |
definition=Not a physical VMS but a conceptual one used in the electronic distribution of information order=6
other | Public | enumerationLiteral
definition=Other than as defined in this enumeration. order=99
Tag | Value
definition | Type of variable message sign.
Details:
Property | Value
isFinalSpecialization: | 0